<tt>
Flag Instructions
</tt>

<ms>
Instructions that enable or disable certain flags always begin with the letter "X" (capital X). In order for these instructions to be executed, the command interpreter must arrive at them, and not be interrupted beforehand (short-circuited).
</ms>

<rl>
</rl>

<ck>
000000000EOJE1
</ck>

<in>

</in>
