<tt>
Insert a line
</tt>

<ms>
Wizard for inserting a line into the tactile graph. You must enter the start and end coordinates of the line:

- Starting point coordinates X1 and Y1: Pair of values that indicate the starting point of the line to be drawn;
- End point coordinates X2 and Y2: Pair of values that indicate the point to which the line to be drawn must lead.
</ms>

<rl>
TBiblosGeometryDot
TBiblosBrailleGeometry
</rl>

<ck>
01HBXY23298WC5
</ck>

<in>
340 0
</in>
