
        +----------------------------------------------------------+
        |    IBM Auto 16/4 Token-Ring ISA Adapter Device Driver    |
        |  Installation instructions for Microsoft Windows NT (TM) |
        +----------------------------------------------------------+


        1.0     PHYSICAL INSTALLATION

            The IBM Auto 16/4 Token-Ring ISA adapter must be
            physically installed and configured before you begin the
            driver installation.  If you have not already installed
            the adapter, please refer to the product documentation
            that was shipped with it.


        2.0     DRIVER INSTALLATION

            The general procedure for installing network device
            drivers for Windows NT is documented in the Microsoft
            Windows NT System Guide (Document No.  36327-0593),
            chapter 5. The main points are summarized below:


            2.1     Log on as an administrator

                In order to make changes to the network, you need to
                be logged on as a member of the administrator group
                for your computer.


            2.2     Select the Main program group

                After you log on to Windows NT, you should see
                several program group icons in the Program Manager
                window.  Select the Main program group by double
                clicking it with the left mouse button.


            2.3     Select the Control Panel application

                Double click on the Control Panel icon.  If for some
                reason the Control Panel icon is missing, you can
                enter "control" on a command line to initiate the
                program directly.  You can get a command line prompt
                by selecting the MS DOS Command Prompt icon.


            2.4     Select the Network application

                Once the Control Panel window is displayed, select
                the Network application.  You should then see a
                Network Settings window having the following buttons:

                Change (Computer Name)
                Change (Workgroup)
                Add Software
                Add Adapter
                Configure
                Update Remove
                OK
                Close
                Bindings
                Networks
                Help

                There should be two list boxes displayed in the lower
                left of the window.  The one on the top is labeled
                "Installed Network Software" and the one on the
                bottom is labeled "Installed Adapter Cards".  The
                bottom one is the only one you will be concerned
                with.  When you are done with installation, this list
                box should contain entries for the adapters you have
                installed.


            2.5     Click on Add Adapter

                When you are ready to begin, click on the "Add
                Adapter ..." button (NOT "Add Software ...").

                You should see the message "Setup is preparing network
                card choices ..." displayed in a window.  This may take
                10 to 30 seconds, depending on your configuration.


            2.6     Select "OTHER"

                After the setup program has located all network card
                choices, it will display a window with the title "Add
                Network Adapter".  In this window, you should see a
                combo box with a number of manufacturers names.
                Click on the down arrow to browse the list.  The last
                selection should be "<Other> Requires disk from
                manufacturer".  Click on this selection to highlight
                it then click on the "CONTINUE" button.


            2.7     Insert the diskette in the A: drive

                You should next see a window with the title "Insert
                Diskette".  Put the IBM Auto 16/4 Token-Ring ISA
                Adapter Device Driver installation diskette in the A:
                drive.  The entry field should already be filled in.
                If it is not, enter "A:\".  When you are ready, click
                on the "OK" button.


            2.8     Select "IBM Auto 16/4 Token-Ring ISA Adapter"
                    software

                When this "Select OEM Option" window is displayed,
                you should see one selection in the list box, "IBM
                Auto 16/4 Token-Ring ISA Adapter".  Click on the "OK"
                button.

                You should next see several work-in-progress windows
                that indicate that the driver and its supporting
                files are being copied to your computer's hard disk.
                This should take about 10 - 20 seconds.  The file
                that is installed should be:

                            IBMTOK4.SYS


            2.9     Enter configuration parameters

                The next window you see will be a dialog box prompting
                you for the network address.  If you will be using a
                locally administered address, enter it in this field.
                If you do not enter a network address, the driver will
                use the burned-in address from the adapter.

                When you are finished examining or modifying the
                parameter values, click on the OK button.


            2.10    Click on OK in Network Settings

                You should see the Network Settings panel again.  This
                time, there should be an entry for the adapter you just
                added in the "Installed Adapter Cards" list box.

                IMPORTANT:  You must click on the OK button at the top
                right of this window to complete the installation.

                After you click on OK, you should shortly see a message
                that indicates you need to shut down and reboot.  By
                responding "YES" to this message, Windows NT will
                automatically shut down and reboot for you.

                When the system comes back up, you should be able to
                log on and use the IBM Auto 16/4 Token-Ring ISA
                adapter.

        ***

        Trademarks

        IBM and IBM Auto 16/4 Token-Ring ISA are trademarks of the IBM Corporation
        in the United States and/or other countries.

        Microsoft, MS-DOS and Windows NT are trademarks of Microsoft
        Corporation in the U.S.A. and other countries.
