[data]
("WIN86.COM")
("")
("C:\WIN386")
("Windows/386")
("Microsoft Windows/386 Version 2.1")
("WIN386")
("")

[diskette]
("Installation 1")
("Installation 2")
("Installation 3")
("Installation 4")
("Installation 5")
("Installation 6")

[windows]
(1:KERNEL.EXE)
(1:GDI.EXE)
(1:USERF.EXE)
(1:MSDOS.EXE)
(4:RAMDRIVE.SYS)

[system]
(1:SYSTEM.DRV)
(1:MSDOSD.EXE)
(1:SOUND.DRV)
(1:COMM.DRV)
(1:WINOLDAP.MOD)
(1:SPOOLER.EXE)

[display]
(2:CGA.DRV,"CGA","200,96,48","1")
(2:EGAHIRES.DRV,"Moniteur couleur EGA avec haute r‚solution","133,96,72","100")
(2:VGA450.DRV,"VGA","100,96,96","101")
(2:HERCULES.DRV,"Moniteur Hercules avec haute r‚solution monochrome","133,96,72","8")
(2:VGA450.DRV,"Quadram QuadVGA, ATI VIP VGA, ou autre Chips and Technologies 82C441-based VGAs","100,96,96","106")

[logos]
(2:CGA.LGO,EGAHIRES.LGO)
(2:CGA.LGO,VGA450.LGO)
(2:CGA.LGO,CGA.LGO)
(2:HERCULES.LGO,HERCULES.LGO)

[oemlogos]
(1:386LOGO.LGD)

[grabber]
(2:EGA.GRB,EGAHIRES.GRB)
(2:VGA.GRB,VGA450.GRB)
(2:CGA.GRB,CGA.GRB)
(2:HERCULES.GRB,HERCULES.GRB)

[386EXE]
(2:EGA.3EX,EGAHIRES.3EX)
(2:EGA.3EX,VGA450.3EX)
(2:CGA.3EX,CGA.3EX)
(2:HERCULES.3EX,HERCULES.3EX)

[386]
(2:EGA.386,EGAHIRES.386)
(2:EGA.386,VGA450.386)
(2:CGA.386,CGA.386)
(2:HERCULES.386,HERCULES.386)

[keyboard]
(1:KBDFR.DRV,"Clavier Fran‡ais",1)
(1:KBDGR.DRV,"Clavier Allemand",1)
(1:KBDUK.DRV,"Clavier Anglais",1)
(1:KBDBE.DRV,"Clavier Belge",1)
(1:KBDCA.DRV,"Clavier Canadien fran‡ais ",4)
(1:KBDDA.DRV,"Clavier Danois",2)
(1:KBDSP.DRV,"Clavier Espagnol (national)",1)
(1:KBDNE.DRV,"Clavier Hollandais",1)
(1:KBDIT.DRV,"Clavier Italien",1)
(1:KBDIC.DRV,"Clavier Icelandic",1)
(1:KBDLA.DRV,"Clavier Latino Am‚ricain",1)
(1:KBDNO.DRV,"Clavier Norv‚gien",2)
(1:KBDPO.DRV,"Clavier Portugais",3)
(1:KBDFS.DRV,"Clavier Su‚dois/Finnois",1)
(1:KBDSG.DRV,"Clavier Suisse/allemand",1)
(1:KBDSF.DRV,"Clavier Suisse/fran‡ais",1)
(1:KBDUS.DRV,"Clavier US",1)

[pointing.device]
(2:NOMOUSE.DRV,"Pas de module de pointage")
(2:HPMOUSE.DRV,"Souris HP (HP-HIL)")
(2:LMOUSE.DRV,"Souris Logitech")
(2:MOUSE.DRV,"Souris Microsoft (Bus/S‚rie)")
(2:MSMOUSE1.DRV,"Mouse Systems Mouse connect‚ … COM1:")
(2:MSMOUSE2.DRV,"Mouse Systems Mouse connect‚ … COM2:")
(2:MOUSE.DRV,"Souris int‚gr‚e")

[sysfonts]
(2:FONTLO.FON,"Police System petite taille (CGA)","200,96,48")
(2:FONTHI.FON,"Police System petite taille (EGA)","133,96,72")
(2:FONTSQ.FON,"Police System taille moyenne (640*400)","120,96,80")
(2:FONTSQ.FON,"Police System taille moyenne (VGA)","100,96,96")

[oemfonts]
(2:FONTLOUS.FON,"Police Terminal petite taille (USA/Europe - CGA)","200,96,48",0)
(2:FONTHIUS.FON,"Police Terminal taille moyenne (USA/Europe - EGA)","133,96,72",0)
(2:FONTSQUS.FON,"Police Terminal grande taille (USA/Europe - 640*400)","120,96,80",1)
(2:FONTSQUS.FON,"Police Terminal grande taille (USA/Europe - VGA)","100,96,96",1)
(2:FONTSQNO.FON,"Police Terminal grande taille (Pays nordiques - 640*400)","120,96,80",2)
(2:FONTSQNO.FON,"Police Terminal grande taille (Pays nordiques - VGA)","100,96,96",2)
(2:FONTSQPO.FON,"Police Terminal grande taille (Portugal- 640*400)","120,96,80",3)
(2:FONTSQPO.FON,"Police Terminal grande taille (Portugal- VGA)","100,96,96",3)
(2:FONTSQCA.FON,"Police Terminal grande taille (Canada Fran‡ais- 640*400)","120,96,80",4)
(2:FONTSQCA.FON,"Police Terminal grande taille (Canada Fran‡ais- VGA)","100,96,96",4)
(2:FONTSQES.FON,"Police Terminal grande taille (Espagne- 640*400)","120,96,80",5)
(2:FONTSQES.FON,"Police Terminal grande taille (Espagne - VGA)","100,96,96",5)

[country]
("France","33!1!3!2!1!1!!!F!.!,!/!:!;")
("Allemagne","49!1!3!2!1!1!!!DM!.!,!.!:!;")
("Argentine","54!1!2!2!1!0!!!A!.!,!-!:!;")
("Australie","61!1!0!2!1!1!!!$!,!.!-!:!,")
("Autriche","43!1!2!2!1!1!!!VS!.!,!.!:!;")
("Belgique","32!1!3!2!1!1!!!F!.!,!/!:!;")
("Br‚sil","55!1!0!2!1!0!!!Cz$!.!,!-!:!;")
("Canada","2!1!0!2!1!0!!!$!.!,!/!:!;")
("Chili","56!0!0!2!1!0!!!$!.!,!-!:!;")
("Danemark","45!1!3!2!1!1!!!Kr!.!,!/!.!;")
("Espagne","34!1!3!2!1!0!!!Pts!.!,!/!:!;")
("Etats-Unis","1!0!0!2!0!0!AM!PM!$!,!.!/!:!,")
("Finlande","358!1!3!2!1!0!!!MK! !,!-!:!;")
("Hollande","31!1!0!2!1!1!!!Fl!.!,!-!.!;")
("Irlande","353!1!0!2!1!0!!!#Ir!,!.!-!:!,")
("Italie","39!1!3!0!1!1!!!L.!.!,!/!:!;")
("Japon","81!2!0!2!0!0!AM!PM!¥!,!.!/!:!,")
("Liban","011!1!3!2!1!0!!!LL! !,!/!:!;")
("Luxembourg","352!1!3!2!1!0!!!F! !,!/!:!;")
("Mexique","52!1!0!2!0!0!!!$!,!.!/!:!,")
("NorvŠge","47!1!3!2!1!1!!!KR!.!,!/!.!;")
("P‚rou","51!0!0!2!1!0!!!S/.!.!,!-!:!;")
("Portugal","351!0!0!2!1!0!!!Esc!.!,!-!:!;")
("Royaume-Uni","44!1!0!2!1!0!!!£!,!.!-!:!,")
("SuŠde","46!2!3!2!1!1!!!kr!.!,!-!.!;")
("Suisse","41!1!2!2!1!1!!!SF!.!,!.!.!;")
("V‚n‚zuela","58!1!2!2!0!1!!!Bs!.!,!-!:!;")

[io.device]
(3:TTY.DRV,"G‚n‚rique/Texte/Daisywheel","DEVICESPECIFIC")
(4:PSCRIPT.DRV,"Agfa/Compugraphic 400PS [Imprimante PostScript]","DEVICESPECIFIC")
(3:EPSON9.DRV,"AMSTRAD DMP [9 pin]","167,120,72","60,72,120")
(3:EPSON24.DRV,"AMSTRAD LQ [24 pin]","100,180,180","67,120,180")
(4:PSCRIPT.DRV,"Apple LaserWriter [Imprimante PostScript]","DEVICESPECIFIC")
(4:PSCRIPT.DRV,"Apple LaserWriter Plus [Imprimante PostScript]","DEVICESPECIFIC")
(4:PSCRIPT.DRV,"Apple LaserWriter II NT/NTX [Imprimante PostScript]","DEVICESPECIFIC")
(3:HPPCL.DRV,"Apricot Laser [PCL / HP LaserJet]","DEVICESPECIFIC")
(4:PSCRIPT.DRV,"AST TurboLaser/PS - R4081 [Imprimante PostScript]","DEVICESPECIFIC")
(3:HPPLOT.DRV,"AT&T 435","CONTINUOUSSCALING")
(4:CITOH.DRV,"AT&T 470/475","133,96,72","75,72,96")
(4:IBMGRX.DRV,"AT&T 473/478","167,120,72","60,72,120")
(4:CITOH.DRV,"C-Itoh 8510","133,96,72","75,72,96")
(4:LBP8US.DRV,"Canon LBP-8 II","DEVICESPECIFIC")
(4:PSCRIPT.DRV,"Dataproducts LZR 2665 [Imprimante PostScript]","DEVICESPECIFIC")
(4:PSCRIPT.DRV,"Digital LN03R ScriptPrinter [Imprimante PostScript]","DEVICESPECIFIC")
(4:PSCRIPT.DRV,"Digital LPS PrintServer 40 [Imprimante PostScript]","DEVICESPECIFIC")
(3:EPSON9.DRV,"Epson EX-800/1000 [Epson 9 pin]","167,120,72","60,72,120")
(3:EPSON9.DRV,"Epson FX-100 [Epson 9 pin]","167,120,72","60,72,120")
(3:EPSON9.DRV,"Epson FX-100+ [Epson 9 pin]","167,120,72","60,72,120")
(3:EPSON9.DRV,"Epson FX-185/286 [Epson 9 pin]","167,120,72","60,72,120")
(3:EPSON9.DRV,"Epson FX-80 [Epson 9 pin]","167,120,72","60,72,120")
(3:EPSON9.DRV,"Epson FX-80+ [Epson 9 pin]","167,120,72","60,72,120")
(3:EPSON9.DRV,"Epson FX-85 [Epson 9 pin]","167,120,72","60,72,120")
(3:EPSON9.DRV,"Epson FX-86e/286e [Epson 9 pin]","167,120,72","60,72,120")
(3:HPPCL.DRV,"[Epson GQ-3500] avec cartouche compatible HP LaserJet","DEVICESPECIFIC")
(3:EPSON9.DRV,"Epson JX-80 [Epson 9 pin]","167,120,72","60,72,120")
(3:EPSON24.DRV,"Epson LQ500 [Epson 24 pin]","100,180,180","67,120,180")
(3:EPSON24.DRV,"Epson LQ800 [Epson 24 pin]","100,180,180","67,120,180")
(3:EPSON24.DRV,"Epson LQ850 [Epson 24 pin]","100,180,180","67,120,180")
(3:EPSON24.DRV,"Epson LQ1000 [Epson 24 pin]","100,180,180","67,120,180")
(3:EPSON24.DRV,"Epson LQ1050 [Epson 24 pin]","100,180,180","67,120,180")
(3:EPSON24.DRV,"Epson LQ1500 [Epson 24 pin]","100,180,180","67,120,180")
(3:EPSON24.DRV,"Epson LQ2500 [Epson 24 pin]","100,180,180","67,120,180")
(3:EPSON9.DRV,"Epson LX-80 [Epson 9 pin]","167,120,72","60,72,120")
(3:EPSON9.DRV,"Epson LX-800 [Epson 9 pin]","167,120,72","60,72,120")
(3:EPSON9.DRV,"Epson LX-86 [Epson 9 pin]","167,120,72","60,72,120")
(3:EPSON9.DRV,"Epson MX-100 [Epson 9 pin]","167,120,72","60,72,120")
(3:EPSON9.DRV,"Epson MX-80/80F/T [Epson 9 pin]","167,120,72","60,72,120")
(3:EPSON9.DRV,"Epson RX-100 [Epson 9 pin]","167,120,72","60,72,120")
(3:EPSON9.DRV,"Epson RX-80/80F/T [Epson 9 pin]","167,120,72","60,72,120")
(3:EPSON24.DRV,"Epson SQ2500 [Epson 24 pin]","100,180,180","67,120,180")
(3:FUJIMTRX.DRV,"Fujitsu DL 2400","167,120,72","60,72,120")
(3:FUJIMTRX.DRV,"Fujitsu DL 2600","167,120,72","60,72,120")
(3:FUJIMTRX.DRV,"Fujitsu DL 3300","167,120,72","60,72,120")
(3:FUJIMTRX.DRV,"Fujitsu DL 3400","167,120,72","60,72,120")
(3:FUJIMTRX.DRV,"Fujitsu DL 5600","167,120,72","60,72,120")
(3:FUJIMTRX.DRV,"Fujitsu DX 2200","167,120,72","60,72,120")
(3:FUJIMTRX.DRV,"Fujitsu DX 2300","167,120,72","60,72,120")
(3:FUJIMTRX.DRV,"Fujitsu DX 2400","167,120,72","60,72,120")
(3:FUJIMTRX.DRV,"Fujitsu DX 3100","167,120,72","60,72,120")
(3:HPPLOT.DRV,"HP 7470A [Traceur HP]","CONTINUOUSSCALING")
(3:HPPLOT.DRV,"HP 7475A [Traceur HP]","CONTINUOUSSCALING")
(3:HPPLOT.DRV,"HP 7550A [Traceur HP]","CONTINUOUSSCALING")
(3:HPPLOT.DRV,"HP 7580A [Traceur HP]","CONTINUOUSSCALING")
(3:HPPLOT.DRV,"HP 7585A [Traceur HP]","CONTINUOUSSCALING")
(3:HPPLOT.DRV,"HP 7580B [Traceur HP]","CONTINUOUSSCALING")
(3:HPPLOT.DRV,"HP 7585B [Traceur HP]","CONTINUOUSSCALING")
(3:HPPLOT.DRV,"HP 7586B [Traceur HP]","CONTINUOUSSCALING")
(3:HPPLOT.DRV,"HP ColorPro [Traceur HP]","CONTINUOUSSCALING")
(3:HPPLOT.DRV,"HP ColorPro avec GEC [Traceur HP]","CONTINUOUSSCALING")
(4:DESKJET.DRV,"HP DeskJet","100,300,300","100,300,300")
(3:HPPLOT.DRV,"HP DraftPro [Traceur HP]","CONTINUOUSSCALING")
(3:HPPLOT.DRV,"HP DraftMaster I [Traceur HP]","CONTINUOUSSCALING")
(3:HPPLOT.DRV,"HP DraftMaster II [Traceur HP]","CONTINUOUSSCALING")
(3:HPPCL.DRV,"HP LaserJet [PCL / HP LaserJet]","DEVICESPECIFIC")
(3:HPPCL.DRV,"HP LaserJet Plus [PCL / HP LaserJet]","DEVICESPECIFIC")
(3:HPPCL.DRV,"HP LaserJet 500+ [PCL / HP LaserJet]","DEVICESPECIFIC")
(3:HPPCL.DRV,"HP LaserJet Series II [PCL / HP LaserJet]","DEVICESPECIFIC")
(3:HPPCL.DRV,"HP LaserJet 2000 [PCL / HP LaserJet]","DEVICESPECIFIC")
(4:PAINTJET.DRV,"HP PaintJet","100,180,180","100,180,180")
(4:THINKJET.DRV,"HP ThinkJet","200,192,96","50,96,192")
(3:IBMCOLOR.DRV,"IBM Color Printer (N/B)","167,140,84","60,84,140")
(3:IBMGRX.DRV,"IBM Graphics","167,120,72","60,72,120")
(4:PSCRIPT.DRV,"IBM Personal Pageprinter [Imprimante PostScript]","DEVICESPECIFIC")
(3:PROPRINT.DRV,"IBM Proprinter [IBM Proprinters]","167,120,72","60,72,120")
(3:PROPRINT.DRV,"IBM Proprinter II [IBM Proprinters]","167,120,72","60,72,120")
(3:PROPRN24.DRV,"IBM Proprinter X24 [IBM Proprinter 24]","100,180,180","67,120,180")
(3:PROPRINT.DRV,"IBM Proprinter XL [IBM Proprinters]","167,120,72","60,72,120")
(3:PROPRN24.DRV,"IBM Proprinter XL24 [IBM Proprinter 24]","100,180,180","67,120,180")
(4:QWIII.DRV,"IBM QuietWriter III","100,120,120","100,120,120")
(3:HPPCL.DRV,"Kyocera F-1010 Laser [PCL / HP LaserJet]","DEVICESPECIFIC")
(4:PSCRIPT.DRV,"Linotronic 100/300/500 [Imprimante PostScript]","DEVICESPECIFIC")
(3:NECP2.DRV,"NEC P2/P3","200,120,60","50,60,120")
(3:NECCOLOR.DRV,"NEC PinWriter CP6 [NEC 24-Wire Pinwriter]","100,360,360","100,360,360")
(3:NECCOLOR.DRV,"NEC PinWriter CP7 [NEC 24-Wire Pinwriter]","100,360,360","100,360,360")
(3:NECCOLOR.DRV,"NEC PinWriter P2200 [NEC 24-Wire Pinwriter]","100,360,360","100,360,360")
(3:NECCOLOR.DRV,"NEC PinWriter P5 [NEC 24-Wire Pinwriter]","100,360,360","100,360,360")
(3:NECCOLOR.DRV,"NEC PinWriter P5XL [NEC 24-Wire Pinwriter]","100,360,360","100,360,360")
(3:NECCOLOR.DRV,"NEC PinWriter P6 [NEC 24-Wire Pinwriter]","100,360,360","100,360,360")
(3:NECCOLOR.DRV,"NEC PinWriter P7 [NEC 24-Wire Pinwriter]","100,360,360","100,360,360")
(3:NECCOLOR.DRV,"NEC PinWriter P9XL [NEC 24-Wire Pinwriter]","100,360,360","100,360,360")
(3:NECCOLOR.DRV,"NEC PinWriter P5200 [NEC 24-Wire Pinwriter]","100,360,360","100,360,360")
(3:NECCOLOR.DRV,"NEC PinWriter P5300 [NEC 24-Wire Pinwriter]","100,360,360","100,360,360")
(3:HPPCL.DRV,"NEC SilentWriter LC 860 [PCL / HP LaserJet]","DEVICESPECIFIC")
(4:PSCRIPT.DRV,"NEC SilentWriter LC 890 [Imprimante PostScript]","DEVICESPECIFIC")
(3:IBMGRX.DRV,"Okidata 92/192 (IBM)","167,120,72","60,72,120")
(3:IBMGRX.DRV,"Okidata 93/193 (IBM)","167,120,72","60,72,120")
(3:OKI24.DRV,"Okidata 390 [Okidata 24 pin]","100,180,180","67,120,180")
(3:OKI24.DRV,"Okidata 391 [Okidata 24 pin]","100,180,180","67,120,180")
(3:OKI24.DRV,"Okidata 393 [Okidata 24 pin]","100,180,180","67,120,180")
(3:OKI24.DRV,"Okidata 393C [Okidata 24 pin]","100,180,180","67,120,180")
(3:HPPCL.DRV,"Okidata LaserLine 6 [PCL / HP LaserJet]","DEVICESPECIFIC")
(4:OLIPRINT.DRV,"Olivetti DM 100/1 [Imprimante Olivetti DM]","167,120,72","60,72,120")
(4:OLIPRINT.DRV,"Olivetti DM 100/2 [Imprimante Olivetti DM]","167,120,72","60,72,120")
(4:OLIPRINT.DRV,"Olivetti DM 100/4 [Imprimante Olivetti DM]","167,120,72","60,72,120")
(4:OLIPRINT.DRV,"Olivetti DM 105 [Imprimante Olivetti DM]","167,120,72","60,72,120")
(4:OLIPRINT.DRV,"Olivetti DM 280/282 [Imprimante Olivetti DM]","167,120,72","60,72,120")
(4:OLIPRINT.DRV,"Olivetti DM 286/296 [Imprimante Olivetti DM]","167,120,72","60,72,120")
(4:OLIPRINT.DRV,"Olivetti DM 290/292 [Imprimante Olivetti DM]","167,120,72","60,72,120")
(4:OLIPRINT.DRV,"Olivetti DM 580 [Imprimante Olivetti DM]","167,120,72","60,72,120")
(4:OLIPRINT.DRV,"Olivetti DM 590 [Imprimante Olivetti DM]","167,120,72","60,72,120")
(3:DM600.DRV,"Olivetti DM 600","100,180,180","67,120,180")
(4:OLIPRINT.DRV,"Olivetti PR 15B/17B [Imprimante Olivetti DM]","167,120,72","60,72,120")
(4:OLIPRINT.DRV,"Olivetti PR 19B [Imprimante Olivetti DM]","167,120,72","60,72,120")
(4:PSCRIPT.DRV,"Olivetti Cicero PG 301","DEVICESPECIFIC")
(4:LBP8US.DRV,"Olivetti PG 208 M1","DEVICESPECIFIC")
(3:HPPCL.DRV,"Olivetti PG 208 M2","DEVICESPECIFIC")
(4:PSCRIPT.DRV,"QMS-PS 800 [Imprimante PostScript]","DEVICESPECIFIC")
(4:PSCRIPT.DRV,"QMS-PS 800 Plus [Imprimante PostScript]","DEVICESPECIFIC")
(3:HPPCL.DRV,"QuadLaser I [PCL / HP LaserJet]","DEVICESPECIFIC")
(3:HPPCL.DRV,"Tandy LP-1000 [PCL / HP LaserJet]","DEVICESPECIFIC")
(3:HPPCL.DRV,"Tegra Genesis [PCL / HP LaserJet]","DEVICESPECIFIC")
(4:TI850.DRV,"TI 850","167,120,72","60,72,120")
(4:TI850.DRV,"TI 855","167,120,72","60,72,120")
(4:PSCRIPT.DRV,"TI OmniLaser 2108 [Imprimante PostScript]","DEVICESPECIFIC")
(4:PSCRIPT.DRV,"TI OmniLaser 2115 [Imprimante PostScript]","DEVICESPECIFIC")
(4:TOSH.DRV,"Toshiba P1350/P1351","300,180,60","33,60,180")
(4:PSCRIPT.DRV,"Varityper VT-600 [Imprimante PostScript]","DEVICESPECIFIC")
(4:PSCRIPT.DRV,"Wang LCS15 [Imprimante PostScript]","DEVICESPECIFIC")
(4:PSCRIPT.DRV,"Wang LCS15 FontPlus [Imprimante PostScript]","DEVICESPECIFIC")
(3:HPPCL.DRV,"Wang LDP8 [PCL / HP LaserJet]","DEVICESPECIFIC")
(4:XER4020.DRV,"Xerox 4020","100,120,120","100,120,120")

[io.dependent]
(5:INFOE2.TXT,EPSON24.DRV)
(5:INFOE9.TXT,EPSON9.DRV)
(5:INFOFU.TXT,FUJIMTRX.DRV)
(5:INFOHP.TXT,HPPCL.DRV)
(5:INFONE.TXT,NECCOLOR.DRV)
(5:INFOO2.TXT,OKI24.DRV)
(5:INFOOL.TXT,OLIPRINT.DRV)
(5:INFOOL.TXT,DM600.DRV)
(5:INFOP2.TXT,PROPRN24.DRV)
(5:INFOP9.TXT,PROPRINT.DRV)
(5:INFOPJ.TXT,PAINTJET.DRV)
(5:INFOPL.TXT,HPPLOT.DRV)
(5:INFOPS.TXT,PSCRIPT.DRV)
(5:A4TRAY.TXT,PSCRIPT.DRV)

[fonts]
(5:ROMAN.FON,"Roman (Set #1)","CONTINUOUSSCALING" )
(5:SCRIPT.FON,"Script (Set #1)","CONTINUOUSSCALING" )
(5:MODERN.FON,"Modern (Set #1)","CONTINUOUSSCALING" )
(5:HELVA.FON,"Helv 8,10,12,14,18,24 (Set #2)","200,96,48" )
(5:HELVB.FON,"Helv 8,10,12,14,18,24 (Set #3)","133,96,72" )
(5:HELVC.FON,"Helv 8,10,12,14,18,24 (Set #4)","83,60,72" )
(5:HELVD.FON,"Helv 8,10,12,14,18,24 (Set #5)","167,120,72" )
(5:HELVE.FON,"Helv 8,10,12,14,18,24 (Set #6)","100,96,96" )
(5:COURA.FON,"Courier 8,10,12 (Set #2)","200,96,48" )
(5:COURB.FON,"Courier 8,10,12 (Set #3)","133,96,72" )
(5:COURC.FON,"Courier 8,10,12 (Set #4)","83,60,72" )
(5:COURD.FON,"Courier 8,10,12 (Set #5)","167,120,72" )
(5:COURE.FON,"Courier 8,10,12 (Set #6)","100,96,96" )
(5:TMSRA.FON,"Tms Rmn 8,10,12,14,18,24 (Set #2)","200,96,48" )
(5:TMSRB.FON,"Tms Rmn 8,10,12,14,18,24 (Set #3)","133,96,72" )
(5:TMSRC.FON,"Tms Rmn 8,10,12,14,18,24 (Set #4)","83,60,72" )
(5:TMSRD.FON,"Tms Rmn 8,10,12,14,18,24 (Set #5)","167,120,72" )
(5:TMSRE.FON,"Tms Rmn 8,10,12,14,18,24 (Set #6)","100,96,96" )

[apps]
(1:CGA40.FON)
(1:CGA80.FON)
(1:EGA40.FON)
(1:EGA80.FON)
(1:HERCULES.FON)
(6:COMMANDE.PIF)
(6:COMMANDP.PIF)
(6:COMMANDF.PIF)
(6:CALC.EXE)
(6:AGENDA.EXE)
(6:REPERT.EXE)
(6:PRESSPAP.EXE)
(6:HORLOGE.EXE)
(6:CONTROL.EXE)
(6:CVTPAINT.EXE)
(6:BLOCNOTE.EXE)
(6:PAINT.EXE)
(6:PIFEDIT.EXE)
(6:REVERSI.EXE)
(6:TERMINAL.EXE)
(6:WRITE.EXE)
(6:ABC.TXT)
(6:SEMAINE.TXT)
(6:EXERCICE.WRI)
(6:LISEZMOI.TXT)
(4:WIN386.PS2)
(4:MEMSET.EXE)
(1:HIMEM.SYS)

[machine]

("AMSTRAD PC avec graphiques VGA et souris int‚gr‚s","101",
SYSTEM.DRV,
KBDFR.DRV,
"Souris int‚gr‚e",
VGA450.DRV,
386LOGO.LGD,
SOUND.DRV,
COMM.DRV,
FONTSQ.FON,
FONTSQUS.FON,
MSDOSD.EXE,
WINOLDAP.MOD,
SPOOLER.EXE)

[harddisk]

[compatibility]
("CEMM.")
("VDISK.")
("CACHE.")
("QEMM.")
("ICACHE.")
("IEMM.")
("ILIM386.")
("386MAX.")
("EMM386.")
