      * * * * * * UPDATED FEATURES FOR AMOUSE VERSION 7.0 * * * * * *

      The following mouse parameters have been added to Amouse driver

     A. Hardware Resolution ( /Rn )
        -------------------------
        With this parameter, an exciting new concept in Mouse control
        has been  developed.  A precise location on the screen can be
        selected with greater ease and speed.

        Movement of the cursor across the screen is based on the tra-
        vel count  and speed of the movement of the mouse.  It is not
        only measured in terms  of physical distance traveled by  the
        mouse, but also checking how quick the mouse is moved by your
        hand.  The faster the movement of the mouse,  the further the
        cursor movement on the screen.  Therefore, less hand movement
        is involved.

        The Mouse's resolution can  be  increased  up  to  4200  dots
        per inch.  You may choose the desired resolution according to
        the requirements of your applications.

        This option is not case sensitive : any combination of upper-
        case and lowercase letter is acceptable.

        To select the resolution, type the command:


        A:>AMOUSE /Rn   ( Where n = 0 to 9, 0 set the auto hardware
                          resolution.)

        For example, if you set the resolution on the double times,
        enter the followings : AMOUSE /R2

     B. Communication Port ( n )
        ------------------------
        There are four general purpose communication ports  generally
        used on your personal computer. The relative address and  IRQ
        no. are listed in the table below:

        -------+----------+------------------+----------
           n   |  COM no. |  Address in HEX. |  IRQ no.
        -------+----------+------------------+----------
           1   |  COM 1   |       3F8h       |  IRQ 4
           2   |  COM 2   |       2F8h       |  IRQ 3
           3   |  COM 3   |       3E8h       |  IRQ 4
           4   |  COM 4   |       2E8h       |  IRQ 3
        -------+----------+------------------+----------

        The Serial Mouse can be set to any one of the four
        communication ports, ( COM1 to COM4 ). The command format is

        A:>AMOUSE /n   ( Where n = 1 to 4 ).

        For example, if you install the mouse at COM1 ( default sett-
        ing ), enter the following:
        A:>AMOUSE /1 or A:>AMOUSE

        If you want to install the mouse at COM4 enter the following:
        A:>AMOUSE/4


     C. Hand Mode
        ---------
        Amouse driver provides two opertion modes for users.One is for
        right-handed users,the other for left-handed users.

        If you are a right-handed user,type following
        A:>AMOUSE  (the driver default setting is right-handed mode)

        If you are a left-handed user,please type following
        A:>AMOUSE/L or AMOUSE/l


     D. Multiple parameters
        -------------------
        It is also possible to select the resolution,the communication
        port and hand mode at the same time. The sequence of selecting
        the multiple parameter is:
        1). Resolution ( /Rn)
        2). Communication port ( /n )
        3). Hand Mode

        The parameters list above have no certain combination.
        If you type
        A:>AMOUSE /l/2/r3
        it the same as
        A:>AMOUSE /r3/l/2

        NOTE:The driver provides default setting that the parameter
             list above you have not selected.

        Ex: A:>AMOUSE /r3/3
        The  I/O  address is COM3(3E8h) and IRQ4 is assigned. The
        movement of cursor is 3 times faster than the movement of
        mouse,and the driver supports right-handed mode.

        Ex: A:>AMOUSE /2/l
        This command connects your mouse to the standard communicat-
        ion port COM2.The driver supports left-haanded mode and the
        movement of cursor becomes 1 times (default setting) hardware
        resolution.

        Ex: A:>AMOUSE /4
        This command connects your mouse to the standard communicat-
        ion port COM4  ( The address and IRQ no.  are found in table
        of section B ) where default hardware resolution is being
        used,and the driver supports right-handed mode.

     E. PS/2 mode
        ---------
        This option tell the mouse driver to install the mouse on a
        mouse port.  Because the first priority of the mouse driver
        installation is the mouse port, the serial ports are choosed
        when a mouse port is unavailable.  This option overrides the
        mouse driver on the mouse port.

        If you use a PS/2 mouse on PS/2 machine,type following
        A:>AMOUSE


     F. BUS mode
        --------
        The Amouse driver also supports BUS mouse,if your BUS mouse
        connnects to a BUS card,then type
        A:>AMOUSE/B or AMOUSE/b


     G. Uninstall ( OFF )
        -----------------
        This option removes the mouse driver from memory.

        Ex : C>AMOUSE OFF

     F. Help ( /H, /h or /? )
        ---------------------
        This option displays all of the options and the command list.
        This option is not case sensitive : any combination of upper-
        case and lowercase letter is acceptable.

