Dedacode PizzaBuffer v2.0 Stereo Buffer-based effect. Parametres: Buffer Lenght: As the word says, this param set the lenght of the Buffer; Repeat: Number of repetitions; Reverse: Number of reversed repetitions sent to output; Silent: Number of silent repetitions sent to output; Fade: Volume of repetitions; Wet Gain: This param set the volume (in %) of the effected signal sent to output; Dry Thru: When the param is set to "0", the buffered signal will be sent to output doing a pause of X ticks (set in Buffer Lenght param) for every cycle; when the param is set to "1", the signal in the buffer will be sent to output without doing any pauses; Dry Gain: This param set the volume (in %) of the clean signal sent to output.
Credits: This machine is distributed as FREEWARE. This documentation is distributed under the terms of GNU Free Documentation License v1.2 or later. Machine Idea + Code: DedaCode Documentation + Skin: ladproject