| # CYANPHASE NOTCH
Type | Effect - Filter
Author | Edward L. Blake (CyanPhase)
Email | blakee@rovoscape.com
Description | The missing piece (i guess) in terms of basic available filters. Also called a band reject, this filter makes a hole in the frequency spectrum at where the Frequency parameter is set.
## PARAMETERS
Fixed1 Filter | This turns the first fixed notch filter on or off.
Fixed1:Freq | Sets the frequency of the notch filter in Hz.
Fixed1:NoteFreq | Sets the frequency of the notch filter with Notes.
Fixed1:BW | Sets the bandwidth of the notch filter (how big the hole the filter makes).
Fixed1:Inertia | Sets how fast the filter moves to the new settings (in units per second, or ticks based on what's set in the attributes).
Fixed2 Filter | This turns the second fixed notch filter on or off.
Fixed2:Freq | Sets the frequency of the notch filter in Hz.
Fixed2:NoteFreq | Sets the frequency of the notch filter with Notes.
Fixed2:BW | Sets the bandwidth of the notch filter (how big the hole the filter makes).
Fixed2:Inertia | Sets how fast the filter moves to the new settings (in units per second, or ticks based on what's set in the attributes).
LFO Filter | This turns the LFO notch filter on or off
LFO:Freq1 | Sets the frequency of the LFO notch filter in Hz, the LFO moves from this point to LFO:Freq2.
LFO:Freq2 | Sets the frequency of the LFO notch filter in Hz, the LFO moves from this point to LFO:Freq1.
LFO:FreqLFO | Sets how fast in seconds per revolution (how long it takes to revolve completely once) the LFO moves between Freq1 and Freq2.
LFO:FreqNote1 | Sets the frequency of the LFO notch filter with Notes, the LFO moves from this point to LFO:Freq2.
LFO:FreqNote2 | Sets the frequency of the LFO notch filter with Notes, the LFO moves from this point to LFO:Freq1.
LFO:BW1 | Sets the bandwidth of the notch filter (how big the hole the filter makes). The LFO moves from this point to LFO:BW2.
LFO:BW2 | Sets the bandwidth of the notch filter (how big the hole the filter makes). The LFO moves from this point to LFO:BW1.
LFO:BW-LFO | Sets how fast in seconds per revolution (how long it takes to revolve completely once) the LFO moves between BW1 and BW2.
## STUFF
E-Mail: | blakee@rovoscape.com.

Copyright © 2000 Edward L. Blake