#

## 3Dizer for Buzz

You ever wished to hear your buzz-tunes with eax enhancement?
So this is for you!

### Idea and Concept

The main idea was, to add dj-tools to buzz.
It should be possible to mix any soundfiles (such mp3) with an external mixtable or anything. For this, we need seperate output channels, to make prelistening possible.
One way is, to support multiple soundcards, but only few people owns 2 or more soundcards, so i looked out for other ways.
I noticed that my sblive has 2 different lineouts, one stereo for the front and another for the rear speakers. It must be possible to misuse theses lineouts.
And now, here is it.

The key is, to use direct sound 3d buffers and setup one to full front and one to full rear.
But I enhanced the idea to eax support, so you have this incredible hardware reverb of the sblive.

So check it out!

### Install and Setup

First download the needed files.

Next unpack the package

- copy wo_eaxout.dll to buzz/WaveOutput
- copy synopia 3DizerListener.dll to buzz/gear/generators
- copy synopia 3DizerBuffer.dll to buzz/gear/effects
- update gear/index.txt

  Now your ready to rock.

- Start buzz, goto View/Preferences
- in the Driver combobox, choose EAX2.0 OUTPUT DRIVER
- click Config
- choose your Soundcard, if the chosen is eax2.0 capable you may enable using EAX2.0
- click ok

- now add one synopia 3DizerListener
- and as much as you want synopia 3DizerBuffer

- connect your machines to the 3DizerBuffers for output
- play around and have fun

  ### Download

- 3Dizer
- EAXUnified-Tool for eax2.0 support

  ### Creds

  Bug report:synopia@gmx.net
  site done with notepad, buzz and psp6.0 in 15min :-)