Dex EFX

thanks to z.war for inspirations

Store it in the effects folder.

This maybe is the most weird effect ever made. It eats a lot of cpu-usage if all is activated (on my PIII-450 up to 27%).
The input- input/auxbus will be "deformt" in up to 5 steps M1/2CombPara1 - M1/2CombPara5.
Each step will be added to the output signal. Furthermore you can add some delay to the output of each matrize.

Here is the layout of the effect:

How to use:

At first choose a channel of the auxbus.

You should select the input of the 2nd matrize -> M2Input
Then you can choose how to "deform" the input of the matrize 1 -> M1Para1 - M1CombPara5
The same you should do with matrize 2 -> M2Para1 - M2CombPara5
With the M1CombM2-slider you choose the combination between the matrizes -> Thru means that only the matrize 1 goes to the output

marc.landis@tokomak.de

Check out http://www.tokomak.de for some music of mine.