DedaCode LaDBox v1.2 Experimental/IDM-oriented FilterBox based on an idea by ladproject. It includes an IIR filter, a LFO, a Highpass and Lowpass Filter and a Gapper. Parametres: Coef b0, Coef b1: IIR Filter parametres. Range: from -1.00 to +1.00. Type LFO: No LFO, Saw, Square, Sin Lenght LFO: 0.001Hz/11ticks Filter: No Filter, HP, LP Cutoff, Resonance: Filter Parametres Lenght Gap: No Gap, 1/7 ticks Wet Gain, Dry Gain: ..
Credits: This machine is distributed as FREEWARE. This documentation is distributed under the terms of GNU Free Documentation License v1.2 or later. Machine Idea + Code: DedaCode Documentation + Skin: ladproject