ase development / buzz plugins
[asedev a4pFilter03] / name

[1.0] / revision
[effect] / type
[15.September.1999] / date of release

Description:
The [asedev a4pFilter03] machine can be used as a resonant 24dB Filter. The user can choose the cutoff and the amount of resonance he wants just by using the two parameters called "Cutoff" and "Resonance". This machine works like the [asedev a2pFilter03] machine except it is more aggressive in the result the user can recieve. If your interested in a less aggressive sound check out the [asedev a2pFilter03] machine. When using extreme settings you might get some heavy distortion.
New in comparison to the [asedev a4pFilter01]:
- from a Cutoff < 100Hz the sound will fadeout (fadeout=cutoff/100).
- from a Cutoff < 50Hz the sound will fadeout (fadeout=(cutoff/100)^2).
- from a Cutoff < 25Hz the sound will stop.
- now the Cutoff will be handled exactly like it should be (maxCutoff = Samplerate / 2).
- this filter can now be used with 96kHz sound output.

Parameters:
Cutoff: The parameter ranges from 1 to 48000. Where a value of 1 is a cutoff frequency of 1Hz and a value of 48000 is a cutoff of 48000Hz. The default cutoff is 5000Hz.
Resonance: The parameter ranges from 1 to 60. Where a value of 1000 results in no resonance and a value of 60000 let the machine get freaky.

Contact:
For feedback and/or bug reports write to asedev@gmx.net

Licensing:
This software is FREEWARE. The author of this program cannot be held responsible for any damage this program may do to your system! Use it at your own risk!