Dedacode Hoffman_Scratch v1.0 Finally a stereo-in/out scratcher effect for Jeskola Buzz :) Parametres: Mono: The effect will be applied only on one input channel (Left or Right) for a low cpu usage, but it will be sent to left and right output channels; Dry Thru: When the param is set to "0", the buffered signal will be sent to output doing a pause of X ticks (set in Lenght param) for every cycle; when the param is set to "1", the signal in the buffer will be sent to output without doing any pauses; Lenght: Lenght of the buffer in ticks; Repeat: This set how many repetitions will be made by the effect engine; Time: This set in % the time of the gap inside every repetition by the formula: Gap = samples in buffer*(Time/100) Space: This set in % the lenght of the buffer segment read in a certain Time. This param is expressed by the formula: buffer segment = samples in buffer*(Space/100) Type: Various algorythms for simulating a kinda-scratch effect!
Credits: This machine is distributed as FREEWARE. This documentation is distributed under the terms of GNU Free Documentation License v1.2 or later. Machine Idea + Code: DedaCode Documentation + Skin: ladproject