# RO-BOT ### What it is RO-BOT is a partially amplitude controlled delay/flanger kind of thing. ### Parameters
Parameter | Description
--- | ---
Pregain | Preamp gain.
Threshold | The threshold. If the signal is louder than this, the delay length begins moving towards the maximum delay. If it's lower, it begins moving towards the minimum.
Level L/R | You can choose to use the auxbus for level input.
Min Delay | Minimum delay.
Max Delay | Maximum delay. Note that this can actually be smaller than the minimum.
Feedback | Feedback. If you use feedbacks above 0 dB, or not far enough below with resonant filters, turn up feedback saturation slightly.
Feedback sign | Feedback positive or negative? Only time will tell.
Feedback sat | Feedback saturation. Causes the delay line to saturate instead of blowing up if positive feedbacks or high filter resonance settings are used.
Filter | Filter mode: Off Lowpass Highpass Bandpass Bandreject (notch).
Cutoff | Filter cutoff frequency.
Resonance | Filter resonance.
C Inertia | Filter cutoff inertia.
Attack | How long it takes the delay time to reach the maximum delay if the signal level stays above the threshold.
Decay | How long it takes the delay time to reach the minimum delay after the signal level drops below the threshold.
LFO Shape | Delay time LFO wave shape: Sine Triangle Square Upsaw Downsaw Random (set at the beginning of each period, with no influence from the L/R phasing) Equal random (set at the beginning of each period, influenced by L/R phasing) Sample and hold (takes the signal level at the beginning of each period and sets the delay length accordingly).
LFO Speed | LFO frequency or period in ticks.
LFO Depth | Depth of the LFO in samples.
LFO Phase | Left/right phase difference of the LFO.
LFO Manual Phase | Sets the LFO to this phase. Useful for synchronizing the LFO with the track.
Manual | Additional manual delay.
M Inertia | Manual delay inertia.
M Inertia Mode | Manual delay inertia mode.
A, B | What to mix with what for the output. D means dry, W means wet.
Mix | Mixing between A and B.
Postgain | Postamp gain.
### Notes & Warnings Be careful with feedbacks near or above 0 dB and filter resonances above 1 if you don't have feedback saturation on. You can use RO-BOT as a vibrato by leaving feedback off, setting minimum and maximum delay to the same value and adjusting the LFO. If the machine blows up on you, you can fix it by right clicking on it and choosing Reset.