Dedacode Hoffman_Scratch v1.0 - Help

Dedacode Hoffman_Scratch v1.0
Finally a stereo-in/out scratcher effect for Jeskola Buzz :)
Parametres:

- Mono:
  The effect will be applied only on one input channel (Left or Right) for a low cpu usage, but it will be sent to left and right output channels;
- Dry Thru:
  When the param is set to "0", the buffered signal will be sent to output doing a pause of X ticks (set in Lenght param) for every cycle; when the param is set to "1", the signal in the buffer will be sent to output without doing any pauses;
- Lenght:
  Lenght of the buffer in ticks;
- Repeat:
  This set how many repetitions will be made by the effect engine;
- Time:
  This set in % the time of the gap inside every repetition by the formula:
  Gap = samples in buffer*(Time/100)
- Space:
  This set in % the lenght of the buffer segment read in a certain Time. This param is expressed by the formula:
  buffer segment = samples in buffer*(Space/100)
- Type:
  Various algorythms for simulating a kinda-scratch effect!

Credits:
This machine is distributed as FREEWARE.
This documentation is distributed under the terms of GNU Free Documentation License v1.2 or later.
Machine Idea + Code: DedaCode
Documentation + Skin: ladproject