Dedacode PizzaBuffer v1.5 - Help

Dedacode PizzaBuffer v1.5
Stereo Buffer-based effect.
Parametres:

- Buffer Lenght:
  As the word says, this param set the lenght of the Buffer;
- Repeat:
  Number of repetitions;
- Reverse:
  Number of reversed repetitions sent to output;
- Silent:
  Number of silent repetitions sent to output;
- Wet Gain:
  This param set the volume (in %) of the effected signal sent to output;
- Dry Thru:
  When the param is set to "0", the buffered signal will be sent to output doing a pause of X ticks (set in Buffer Lenght param) for every cycle; when the param is set to "1", the signal in the buffer will be sent to output without doing any pauses;
- Dry Gain:
  This param set the volume (in %) of the clean signal sent to output.

Credits:
This machine is distributed as FREEWARE.
This documentation is distributed under the terms of GNU Free Documentation License v1.2 or later.
Machine Idea + Code: DedaCode
Documentation + Skin: ladproject