Static Duafilt v1.0 help

Description:
The Static Duafilt is an implementation of Arguru's famous Guru filter in a dual setup. Basically the sound passes through a Low Pass Filter with it's own cutoff and resonance settings and then is passed on to a High Pass filter also with it's own settings.
Paramaters:
LP Cutoff: This sets your Low Pass Cutoff from 0 to 100%.
LP Res: This controls the Resonance (or Q) setting of the Low Pass - 0 to 100%.
HP Cutoff: This sets your High Pass Cutoff from 0 to 100%
HP Res: This controls the Resonance (or Q) setting of the High Pass - 0 to 100%.
Inertia: This sets how many ticks it takes for the Cutoff settings to "catch up" to what you set. Use this for long sweeps etc. - 1 to 1024 ticks