Altering the Amplification (Signal) between machines

Figure 3.7

Follow these steps to quickly alter the gain between two machines: 1. Click on the triangle located between two connected machines.
2. Do not release the mouse button
3. Move the mouse up to raise the amplification or down to lower it.
Tips:
Automating: Amplification may also be automated by scripting it in the destination machine's patterns. For example if an 808 was linking to a reverb, the 808's amplification could be scripted (AKA tracked) by creating a pattern for the reverb, selecting the a-808 column and script as usual.
More Volume: If the maximum volume is not enough for your needs, consider adding one of the gain machines (i.e. asedev Gain01) between a generator and effect (or even two effects).
Recording: The amplification of a machine may be recorded like any other parameter, but you must first create a pattern and column for the destination machine, to allow the movement to be scripted.
Logarithmic Values: The value of the amplification bar in Buzz uses Logarithmic values as opposed to linear. This means that greater changes in the sound will occur toward the bottom of the bar. This is common to traditional music gear and software, and will sound very familiar while used.