DedaCode LaDBox v1.2 - Help

DedaCode LaDBox v1.2
Experimental/IDM-oriented FilterBox based on an idea by ladproject.
It includes an IIR filter, a LFO, a Highpass and Lowpass Filter and a Gapper.
Parametres:

- Coef b0, Coef b1:
  IIR Filter parametres. Range: from -1.00 to +1.00.
- Type LFO:
  No LFO, Saw, Square, Sin
- Lenght LFO:
  0.001Hz/11ticks
- Filter:
  No Filter, HP, LP
- Cutoff, Resonance:
  Filter Parametres
- Lenght Gap:
  No Gap, 1/7 ticks
- Wet Gain, Dry Gain:
  ..

Credits:
This machine is distributed as FREEWARE.
This documentation is distributed under the terms of
GNU Free Documentation License v1.2 or later.
Machine Idea + Code: DedaCode
Documentation + Skin: ladproject