<tt>
Insert the braille type
</tt>

<ms>
Wizard for insert the type of Braille with which to draw a Braille text in the graph.

- Table: From this box you choose which braille table to use to encode the entered text.
- Dot Distance: This value indicates how many pixels should be spaced from one Braille point to the other. The minimum value is 1. For example, if you increase the value to 2, the braille cell points will be more spaced.
- Cell Distance: This value indicates how many pixels are spaced between braille cells.

Always consider that the braille text within a graph is reproduced using the graphics mode (for printers that allow it). Therefore, the distance between the Braille dots may be different from the normal distance because it depends on the tactile resolution of the printer.
</ms>

<rl>
TBiblosGeometryBraille
TBiblosBrailleGeometry
</rl>

<ck>
000SL8PH30ZVDJ
</ck>

<in>
10 0
</in>
