DedaCode SFilterFIR v1.0 Impulse-based / frequencies manipulation effect. Parametres: Coefa0..Coefa4: These params are based on the following math formula: output(t)=input(t)*a0+input(t-1)*a1+input(t-2)*a2+input(t-3)*a3+input(t-4)*a4
Credits: This machine is distributed as FREEWARE. This documentation is distributed under the terms of GNU Free Documentation License v1.2 or later. Machine Idea + Code: DedaCode Documentation + Skin: ladproject