cheapo spread 1.0 [effect]

--------------------------------------------------------------

Usage:
- connect it as normal
- tweak parameters

Not too hard to use is it ;)

Purpose:

To widen the stereo image of a sound.

Features:

- Mono/Stereo
- Per channel (left and right) gain controls (= pan, but with
  more control)
- Phase inversion per channel (left and right). Causes an 
  180 inversion to the selected channels.
- Spread. Variable delay from 1 sample to as-much-as-the-user-
  has-memory for either left or right.
- Shows delay timing values as milliseconds [ms], samples,
  meters or ticks.
--------------------------------------------------------------

I think the parameter and attributes are pretty self-
explaining so you'll have to figure out them your self.

--------------------------------------------------------------
When using machines that change the stereo change, you need to
keep in mind few things:

- It'll sound funny if someone hits the "mono"-switch on their
equipment while listening to the track. If you inverse left
channel and let the right channel be the way it is and you make
a mono signal from the result you'll get silence.
If you put a slight delay to the other channel and that is
monofied, you'll hear two times the hit-sound from hihats and
similar sounds.
- For vinyl you'll want to avoid stereofying sounds with bass
frequencies as in the worse case the needle might jump of the
track because of too much stereo bass.


--------------------------------------------------------------
History:
1.0	First release

--------------------------------------------------------------

oh.. almost forgot: YOU NEED BUZZ1.2 TO USE THIS EFFECT

Mikko Apo [http://iki.fi/apo/]
