Joachim's Hyperion filter (07-May-07) | Planet Filter Series

## Hyperion

30-band Graphical Equalizer for Buzz.
Enable
Bypass switch so that you can easily compare what you did with the original.
Input gain
Signal volume of input into the EQ.
Highpass freq.
For removing unwanted subsonics and DC offset. When set to the lowest value, the highpass filter is disabled to preserve CPU.
Frequency bands
Each frequency band goes from -18 dB to +18 dB and is completely disabled when set to 0 dB to preserve CPU and audio quality.
Bandwidth
The bandwidth of each of the 30 frequency bands. If in doubt just leave this to the default value.

DISCLAIMER: Minimum samplerate: 44100 Hz (and higher is better) This software may be distrbuted freely. The author of this software cannot be held responsible for any damage caused directly or indirectly by using this software.