Venus v1.1

Joachim's Venus filter (30-May-04) | Planet Filter Series

The overall purpose of this effect, is to give you control over the stereo perspective and to add variation and life to the signal.
The sound travels in from the top of this plugin and downwards through the different functions. So the stereo spreader is the first process the sound goes through, and the panning is last.

## Pre stereo:

This is a stereo spreader. At 0 you have mono, at 100% the signal is untouched. At more than 100% the amount of stereo will increase.

## Phaser speed:

The "Phaser" as i call it, is a set of moving EQs that when boosting in one side, they cut in the other side, to get maximum stereo effect.

## Phaser amount:

This is the mix amount of the phaser. At 0.0 dB it is disabled.

## Chorus depth:

Detuning amount of the chorus. At very low values, you can get stranger-like effects. Normal chorusing at anything from 30 to 100, and above that you can get strange horror-like detuning effects. You can also achieve some reverb-like effects using this chorus.

## Chorus amount:

Dry - wet mix between original and chorused signal. The somewhat CPU intensitive chorus is disabled when Chorus amount is at "0".

## EQ mono treble / mid / bass:

This is a normal simple 3-band equalizer. I thought this was convenient to have.

## EQ stereo treble / mid / bass:

These three sliders adjust how much stereo is present at high, mid and low frequencies.

## Randomizer amount:

The randomizer is a strange EQ that gradually boosts different frequencies at a random position in the stereo perspective. The Randomizer is disabled when set to 0.0 dB.

## Randomizer speed:

How fast the randomizer works.

## Stereo limiter:

A rather unique feature that makes sure that the stereo perspective is always below a certain amount. This means that if the incoming signal has a little stereo, nothing will be changed. But if the incoming signal has a lot of stereo, the Stereo limiter will make the stereo perspective more narrow and monoish. Typically you would turn up the "Pre stereo" a little, when using this effect, to compensate for the stereo lost by using this effect.
Technical explanation: The signal is transformed into M-S stereo, and this is a compressor/limiter on the S part of the signal.

## Panning:

A normal panning thingie.

Plug-in written by Joachim Michaelis Homepage | Latest machines | VUmeter.exe

DISCLAIMER: This software may be distrbuted freely. The author of this software cannot be held responsible for any damage caused directly or indirectly by using this software.